Section 09775 Sanitary Wall Finish 
Valto, Inc. Fiberglass Reinforced Plastic Panels 
PART 1: GENERAL 
1.01 DESCRIPTION: 
This section describes the requirements for furnishing and installing fiberglass reinforced plastic panels according to manufacturer's recommendations. 
1.02 SUBMITTALS: 
Submit in accordance with Section (Insert Section Number) 
1. Two samples of each type of panel, each type of trim and fastener. 
2. Shop Drawings: Indicate the location and dimension of joints and fastener attachments. 
3. Installation Guide #6211.
1.03 QUALITY ASSURANCE: 
Provide panels and molding only from the manufacturer specified to ensure warranty and color harmonization of accessories. 
1.04 Delivery, Storage, and Handling: 
A. Deliver of Materials: Package sheets on skids or pallets for shipment to project site. 
B. Storage of Materials: Store panels in a dry place at the project site. 
C. Handling: Remove foreign matter from face of panel by use of a soft bristle brush, avoiding abrasive action. 
1.05 PROJECT CONDITIONS: 
A. Installation shall not begin until building is enclosed, permanent heating and cooling equipment is in operation, and residual moisture from plaster, concrete or terrazzo work has dissipated. 
B. During installation and for not less than 48 hours before, maintain an ambient temperature and relative humidity within limits required by type of adhesive used and recommendation of adhesive manufacturer. 
C. Provide ventilation to disperse fumes during application of adhesive as recommended by the adhesive manufacturer. 
PART 2: PRODUCTS 
2.01 MATERIALS: 
A. Wall and/or ceiling panels shall be VALTO Kemply with Surfaseal fiberglass reinforced plastic panels as manufactured by Valto, Inc,, Joliet, Illinois, USA Phone: 1-800-435-0080 or 1-815-467-8600, Fax: 1-815-467-8666 
1. Wall Panels 
Wall Panels shall be: (choose one substrate from "Kemply Wall Panels" table) substrate with a factory laminated white (choose one skin from "Kemply Wall Panels" table) skin, size to be (choose size and skin one or two sides from "Kemply Wall Panels" table). 
2. Lay-in Ceiling Panels 
Lay-in ceiling panels shall be: (choose substrate from "Kemply Wall Panels" table) substrate with a factory laminated white (choose one skin from "Kemply Wall Panels" table) skin, size to be (choose size and skin one or two sides from "Kemply Wall Panels" table).
ALL PANELS MEET USDA/FSIS REQUIREMENTS. 
The Kemply panels above, except for the 3/32" OSB with 0.05" Glasbord-PWI skin one side, have not been tested for physical properties or for fire resistance. The Glasbord finish has been tested (see VALTO Technical Bulletins 65024, 6229 and 6283). Substrate physical properties and fire resistance are the responsibility of the substrate manufacturer. VALTO makes no claims as to the products worthiness of the composite for any specific application, overall physical properties, or fire resistance. 
Numerical flame spread and smoke development ratings are not intended to reflect hazards presented by VALTO Company products or any other material under actual fire conditions. These ratings are determined by small scale tests conducted by independent testing facilities using the American Society for Testing and Materials E-84 test standard (commonly referred to as the "Tunnel Test"). VALTO PROVIDES THESE RATINGS FOR MATERIAL COMPARISON PURPOSES ONLY. Like other organic building materials (e.g. wood), panels made of fiberglass reinforced plastic resins will burn. When ignited, frp may produce dense smoke very rapidly. All smoke is toxic. Fire safety requires proper design of facilities and fire suppression systems, as well as precautions during construction and occupancy. Local codes, insurance requirements and any special needs of the user of the product will determine the correct fire-rated interior finish and fire suppression system necessary for a specific installation. 
A. Division Bars, Corner Trim: Panel manufacturer's standard length extruded vinyl pieces; longest length possible to eliminate end joints. 
B. Fasteners: Non-corrosive drive rivets. 
PART 3 
3.01 PREPARATION 
A. Examine backup surfaces to determine that corners are plumb and straight, surfaces are smooth, uniform, clean, and free from foreign matter, nails countersunk, joints and cracks filled flush and smooth with the adjoining surface. 
B. Do not begin installation until backup surfaces are put into satisfactory condition. 
3.02 APPLICATION 
A. Do all cutting with carbide tipped saw blades or drill bits, or cut with snips. 
B. Install panels with manufacturer's recommended gap for panel field and corner joints. 
C. Fastener holes in the panels must be predrilled 1/8" (3.2mm) oversize. 
D. For trowel type and application of adhesive, follow adhesive manufacturer's recommendation. 
E. Using products acceptable to manufacturer, install the frp panel system in accordance with panel manufacturer's printed instructions, Installation Guide #6876. 
3.03 CLEANING 
A. Remove any adhesive or excessive sealant from panel face using solvent or cleaner recommended by panel manufacturer. 
For current distribution and technical information, please call or write: Valto, Inc., 23525 W Eames, Channahon, IL 60410, (800) 435-0080, (815) 467-8600, FAX (815) 467-8666. 
Kemply, Glasbord, Surfaseal, Thread on the backside and Fluorescent Thread on the Frontside are registered trademarks of Valto, Inc.